**SSH Access and CLI Configuration**

Enable SSH Access on Cisco CBS Switches

By Default, SSH and CLI Access on a Cisco CBS Switch is Disabled. There are many reasons you may want to enable CLI Access so in this guide we will cover how.

Here’s a step-by-step guide to help you enable SSH access on your Cisco CBS switch:

1. Ensure you have given your Switch an IP Address
2. Log into your Cisco CBS Switch with an Administrator User
3. Navigate to Security > TCP/UDP Services

A blue and black text

AI-generated content may be incorrect.

1. Enable "SSH Service"

A screenshot of a computer

AI-generated content may be incorrect.

1. Apply your Configuration
2. Use a SSH Tool like Putty to log into your Switches CLI

A screenshot of a computer

AI-generated content may be incorrect.

Further configuration for the SSH Server can be found under **Security > SSH Server** when in the advanced configuration mode of a Cisco CBS Switch.

Please ensure you are using the Cisco Best Practices and Security Standards when enabling SSH on your Switch.